# Fibaro Input Plugin

This plugin gathers data from devices connected to a [Fibaro][fibaro]
controller. Those values could be true (1) or false (0) for switches, percentage
for dimmers, temperature, etc. Both _Home Center 2_ and _Home Center 3_ devices
are supported.

⭐ Telegraf v1.7.0
🏷️ iot
💻 all

[fibaro]: https://www.fibaro.com

## Global configuration options <!-- @/docs/includes/plugin_config.md -->

In addition to the plugin-specific configuration settings, plugins support
additional global and plugin configuration settings. These settings are used to
modify metrics, tags, and field or create aliases and configure ordering, etc.
See the [CONFIGURATION.md][CONFIGURATION.md] for more details.

[CONFIGURATION.md]: ../../../docs/CONFIGURATION.md#plugins

## Configuration

```toml @sample.conf
# Read devices value(s) from a Fibaro controller
[[inputs.fibaro]]
  ## Required Fibaro controller address/hostname.
  ## Note: at the time of writing this plugin, Fibaro only implemented http - no https available
  url = "http://<controller>:80"

  ## Required credentials to access the API (http://<controller/api/<component>)
  username = "<username>"
  password = "<password>"

  ## Amount of time allowed to complete the HTTP request
  # timeout = "5s"

  ## Fibaro Device Type
  ## By default, this plugin will attempt to read using the HC2 API. For HC3
  ## devices, set this to "HC3"
  # device_type = "HC2"
```

## Metrics

- fibaro
  - tags:
    - deviceId (device id)
    - section (section name)
    - room (room name)
    - name (device name)
    - type (device type)
  - fields:
    - batteryLevel (float, when available from device)
    - energy (float, when available from device)
    - power (float, when available from device)
    - value (float)
    - value2 (float, when available from device)

## Example Output

```text
fibaro,deviceId=9,host=vm1,name=Fenêtre\ haute,room=Cuisine,section=Cuisine,type=com.fibaro.FGRM222 energy=2.04,power=0.7,value=99,value2=99 1529996807000000000
fibaro,deviceId=10,host=vm1,name=Escaliers,room=Dégagement,section=Pièces\ communes,type=com.fibaro.binarySwitch value=0 1529996807000000000
fibaro,deviceId=13,host=vm1,name=Porte\ fenêtre,room=Salon,section=Pièces\ communes,type=com.fibaro.FGRM222 energy=4.33,power=0.7,value=99,value2=99 1529996807000000000
fibaro,deviceId=21,host=vm1,name=LED\ îlot\ central,room=Cuisine,section=Cuisine,type=com.fibaro.binarySwitch value=0 1529996807000000000
fibaro,deviceId=90,host=vm1,name=Détérioration,room=Entrée,section=Pièces\ communes,type=com.fibaro.heatDetector value=0 1529996807000000000
fibaro,deviceId=163,host=vm1,name=Température,room=Cave,section=Cave,type=com.fibaro.temperatureSensor value=21.62 1529996807000000000
fibaro,deviceId=191,host=vm1,name=Présence,room=Garde-manger,section=Cuisine,type=com.fibaro.FGMS001 value=1 1529996807000000000
fibaro,deviceId=193,host=vm1,name=Luminosité,room=Garde-manger,section=Cuisine,type=com.fibaro.lightSensor value=195 1529996807000000000
fibaro,deviceId=200,host=vm1,name=Etat,room=Garage,section=Extérieur,type=com.fibaro.doorSensor value=0 1529996807000000000
fibaro,deviceId=220,host=vm1,name=CO2\ (ppm),room=Salon,section=Pièces\ communes,type=com.fibaro.multilevelSensor value=536 1529996807000000000
fibaro,deviceId=221,host=vm1,name=Humidité\ (%),room=Salon,section=Pièces\ communes,type=com.fibaro.humiditySensor value=61 1529996807000000000
fibaro,deviceId=222,host=vm1,name=Pression\ (mb),room=Salon,section=Pièces\ communes,type=com.fibaro.multilevelSensor value=1013.7 1529996807000000000
fibaro,deviceId=223,host=vm1,name=Bruit\ (db),room=Salon,section=Pièces\ communes,type=com.fibaro.multilevelSensor value=44 1529996807000000000
fibaro,deviceId=248,host=vm1,name=Température,room=Garage,section=Extérieur,type=com.fibaro.temperatureSensor batteryLevel=85,value=10.8 1529996807000000000
```
