---
title: Worked Examples Using Calico-based OpenStack
canonical_url: 'https://docs.projectcalico.org/v2.6/getting-started/openstack/tutorials'
---

Here are a few worked examples for common {{site.prodname}} on OpenStack deployment
scenarios. In particular, this will make it easy for
you to set up topologies and examine their connectivity to try to get an
understanding of the way {{site.prodname}} networks behave.

## Example 1: Development Machine

In this example, a user wants to spin up a machine to use as a Linux
development environment. This user has a straightforward use-case: they
want a GUI and SSH access, but relatively little else.

This user is provisioned with a single OpenStack user and single
OpenStack tenant. Neutron will automatically provision them with a
single security group, `default`, that contains the following rules:

-   allow all inbound traffic from machines in the `default` security
    group
-   allow all outbound traffic to anywhere

Per the instructions in [this document]({{site.baseurl}}/{{page.version}}/getting-started/openstack/connectivity), this user cannot create
Neutron networks or subnets, but they do have access to the networks
created by the administrator: `external` and `internal`.

Because the user wants to be able to reach the machine from their own
laptop, they need the machine to be reachable from outside the data
center. In vanilla Neutron, this would mean provisioning it with a
floating IP, but in {{site.prodname}} they instead want to make sure the VM is
attached to the `external` network. To add themselves to this network,
the user needs to find out the UUID for it:

```
$ neutron net-list
+--------------------------------------+----------+----------------------------------------------------------+
| id                                   | name     | subnets                                                  |
+--------------------------------------+----------+----------------------------------------------------------+
| 8d5dec25-a6aa-4e18-8706-a51637a428c2 | external | 54db559c-5e1d-4bdc-83b0-c479ef2a0ead 172.18.208.0/24     |
|                                      |          | cf6ceea0-dde0-4018-ab9a-f8f68935622b 2001:db8:a41:2::/64 |
| fa52b704-7b3c-4c83-8698-244807352711 | internal | 301b3e63-5324-4d62-8e22-ed8dddd50689 10.65.0.0/16        |
|                                      |          | bf94ccb1-c57c-4c9a-a873-c20cbfa4ecaf 2001:db8:a41:3::/64 |
+--------------------------------------+----------+----------------------------------------------------------+
```

As the user can see, the `external` network has the UUID
`8d5dec25-a6aa-4e18-8706-a51637a428c2`. Thus, they create the machine
with the following nova boot command:

```
$ nova boot --flavor m1.medium                                  \
            --image debian-wheezy-amd64                         \
            --security-groups default                           \
            --nic "netid=8d5dec25-a6aa-4e18-8706-a51637a428c2"  \
            development-server
```

This places the VM with a single NIC in the `external` network. The VM
starts to boot, and Neutron allocates it an IP address in the `external`
network: in this case, both an IPv4 and IPv6 address, as you can see
below:

```
+--------------------------------------+-----------------------------------------------------------+
| Property                             | Value                                                     |
+--------------------------------------+-----------------------------------------------------------+
| external network                     | 2001:db8:a41:2::1c, 172.18.208.85                         |
| flavor                               | m1.medium (3)                                             |
| hostId                               | b80247c27400fc9048ca569c8635f00801654bf676a00d8f08887215  |
| id                                   | e36f4e62-0efa-4188-87b8-8c96dc6e6028                      |
| name                                 | development-server                                        |
| security_groups                      | default                                                   |
+--------------------------------------+-----------------------------------------------------------+
```

While the machine boots, this tenant decides to configure their security
group. It needs four extra rules: one for SSH and three for VNC. This
developer's personal machine has the IPv4 address 191.64.52.12, and
that's the only machine they'd like to be able to access their machine.
For that reason, they add the four security group rules:

```
$ neutron security-group-rule-create --protocol tcp                      \
                                     --port-range-min 22                 \
                                     --port-range-max 22                 \
                                     --direction ingress                 \
                                     --remote-ip-prefix 191.64.52.12/32  \
                                     --ethertype IPv4                    \
                                     default

$ neutron security-group-rule-create --protocol tcp                      \
                                     --port-range-min 5800               \
                                     --port-range-max 5801               \
                                     --direction ingress                 \
                                     --remote-ip-prefix 191.64.52.12/32  \
                                     --ethertype IPv4                    \
                                     default

$ neutron security-group-rule-create --protocol tcp                      \
                                     --port-range-min 5900               \
                                     --port-range-max 5901               \
                                     --direction ingress                 \
                                     --remote-ip-prefix 191.64.52.12/32  \
                                     --ethertype IPv4                    \
                                     default

$ neutron security-group-rule-create --protocol tcp                      \
                                     --port-range-min 6000               \
                                     --port-range-max 6001               \
                                     --direction ingress                 \
                                     --remote-ip-prefix 191.64.52.12/32  \
                                     --ethertype IPv4                    \
                                     default
```

At this stage, the developer's machine is up and running. It can be
reached on its public IP (172.18.208.85), and the developer confirms
this by SSHing into their box. They're now ready to go.
